**Script**

**R1**

ip access-list standard ADMIN\_VTY

 permit 192.168.2.50

line vty 0 4

 access-class ADMIN\_VTY in

**R2**

access-list 10 remark ACL\_TO\_PINK\_LAN

access-list 10 permit host 192.168.2.50

access-list 10 permit 192.168.1.0 0.0.0.127

access-list 10 permit 172.16.1.0 0.0.0.255

access-list 20 remark ACL\_TO\_BLUE\_LAN

access-list 20 permit host 192.168.1.100

access-list 20 deny 192.168.1.0 0.0.0.255

access-list 20 permit any

interface gigabitEthernet0/0

 ip access-group 20 out

interface gigabitEthernet0/1

 ip access-group 10 out